*) 2-WAY POWERED LINE ARRAY SYSTEM

1. 개요

본 기기는 2-Way 앰프 내장형 라인어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

MILAN 네트워크 AV 시스템

여러가지 소스를 데이지 체인 방식으로 연결

소프트웨어를 통한 모니터링

2x ND7-LM16 7” Kevlar Neodymium Driver

Adamson NH3 3” Diaphragm / 1.4” Exit Compression Driver

100° x 12.5°(H x V) 지향각

해양 등급 자작나무 합판 및 항공기 등급의 강철과 알루미늄으로 제작된 캐비닛

SlideLock 연결 시스템

3. 규격 및 사양

Frequency Range (+/- 3dB)	: 80 Hz - 18 kHz

Nominal Directivity (-6 dB) H x V	: 100° x 12.5°

Maximum Peak SPL	: 138 dB

Components LF	: 2x ND7-LM16 7” Kevlar Neodymium Driver

Components HF	: Adamson NH3 3” Diaphragm / 1.4” Exit	Compression Driver

Rigging	: Slidelock Rigging System

Connections

Power	: powerCON TRUE1

Network	: 2 x etherCON

Analog	: 2 x XLR

Height Front (mm / in)	: 203 / 8

Height Back (mm / in)	: 122 / 4.8

Width (mm / in)	: 527 / 20.75

Depth (mm / in)	: 411 / 16.2

Weight (kg / lbs)	: 17.5 / 38.6

Amplification	: 2 channel Class-D, 2400 W total output

Input Voltage	: 100 - 240 V

Current Draw at 230 V	: 0.45 A rms idle, 1.6 A rms long-term, 9 A max

peak

Processing	: Onboard / Proprietary

* CS7 동급이상품