*) LINE MIXER

1. 개요

본 기기는 12채널 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

6 HDHQ™ Combination inputs with MIC, Phantom and Line selector switches

6 mono (3 stereo) RCA Inputs

Mic monitor ¼” output for private listening to all mic inputs

Balanced XLR line outputs

Mono ¼” line output can be used to feed audio to external recording device

AC or 24V DC power inputs

Mic 1 Priority Control

Master and Individual level controls

1U rack mountable

3. 규격 및 사양

Mic/Line Inputs (Channels 1–6)

- Microphone Input	: XLR+1/4” (6.35 mm) combination, electronically

balanced, discrete input configuration

- Frequency Response	: 20 Hz – 22 kHz (+2 dBu)

- THD+N	: < 0.03% @ 1 kHz

- Sensitivity	: -40 dBu

- Maximum Input	: -19 dBu

- Maximum Voltage Gain	: 60 dB (Mic Input to Line Out, Mic Out & Mono	Out)

: 50 dB (Mic Input to Rec Out)

- Signal-to-Noise Ratio	: > 103 dB

- Phantom Power	: +18–21 V, switch control

Line Inputs (Channels 1–6)

- Line Input	: XLR+1/4” (6.35 mm) combination, electronically

balanced

- Frequency Response	: 20 Hz – 22 kHz (+2 dBu)

- THD+N	: < 0.03% @ 1 kHz

- Sensitivity	: 0 dBu

- Maximum Input	: +21 dBu

- Maximum Voltage Gain	: 20 dB (Mic Input to Line Out, Mic Out & Mono	Out)

: 10 dB (Mic Input to Rec Out)

- Signal-to-Noise Ratio	: > 103 dB

Line Inputs (Channels 7/8–11/12)

- Line Input	: Stereo RCA pairs, electronically balanced

- Frequency Response	: 20 Hz – 22 kHz (+2 dBu)

- THD+N	: < 0.03% @ 1 kHz

- Sensitivity	: +10 dBu

- Maximum Input	: +21 dBu

- Maximum Voltage Gain	: 10 dB (Line Input to Line Out)	: 0 dB (Line Input to Rec Out)

: 4 dB (Line Input to Mono Out)

- Signal-to-Noise Ratio	: > 103 dB

Impedance

- Mic/Line Input	: 1.4 kΩ

- Line Input	: > 10 kΩ

- All Outputs	: 120 Ω

Equalizer

- High	: +15 dB @ 12 kHz

- Mid	: +12 dB @ 2.5 kHz

- Low	: +15 dB @ 80 Hz

Crosstalk

- Adjacent Inputs	: < -70 dB @ 1 kHz (Channels 1–6)	: < -68 dB @ 1 kHz (Channels 7/8–11/12)

- Input to Output	: < -82 dB @ 1 kHz

Main Mix

- Line Output	: 0 dBu (+2 dBu), balanced

- Mic Output, Mono Output	: 0 dBu (+2 dBu), unbalanced

Maximum Output	: +21 dBu balanced/unbalanced, 1/4” jacks

Noise (Bus)	: < -83 dB @ 20 Hz – 22 kHz

Power Connection	: IEC

Dimensions (WxDxH)	: 483 x 195 x 44 mm

Weight	: 2.9kg

* DN-312X 동급이상품