*) MEDIA PLAYER

1. 개요

본 기기는 CD, USB, 블루투스 등을 연결하여 음원 소스를 재생하는 플레이어로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Media player with Network and RS-232C control

Intuitive Web Browser and Infrared user interface

File playback from CD, USB, Network Audio, Bluetooth and AUX

Tempo control for CD and USB

10-track hot start buttons for CD, USB and NET playback

Two Bluetooth antennas included

3. 규격 및 사양

Compatible Media	: CD, 3.5mm auxiliary device, Type A USB	device (mass storage class),	Network-connected device (via Ethernet port),	Bluetooth audio

Supported Device Formats, File Systems

- CD	: CD-DA, CD-ROM (ISO9660), CD-R

- USB	: FAT16, FAT32

Supported File Formats

- CD-DA	: 44.1/48kHz, 16/24 bit

- WAV	: 44.1/48kHz, 16/24 bit

- MP3	: 44.1kHz, 32 kbps to 320 kbps, CBR and VBR

Number of Channels	: 2 (stereo)

Audio Frequency Range	: 10 Hz - 20 kHz (± 1.0db)

Signal-to-Noise Ratio	: > 90dB (A-weighted)

Total Harmonic Distortion	: < 0.01%

Dynamic Range	: > 85dB

Channel Separation	: > 80dB

Bluetooth Version	: 4.0

Analog Out L/R (unbalanced)

- Type	: RCA terminal

- Load impedance	: > 10 kΩ

- Output level	: 2 Vrms @ 10 kΩ load

Analog Out L/R (balanced)

- Type	: XLR

- Load impedance	: > 10 kΩ

- Output level	: +4 dBu

Aux in

- Type	: 1/8" (3.5mm) TRS terminal

- Input Impedance	: > 10 kΩ

- Maximum input level	: 1 Vrms

Remote Control

- Included Remote	: Infrared protocol: NEC format

: Transmit output level : >200mVp-p

- Serial Remote(D-sub 9-pin female RS-232C), Not Included

: Mode: Full duplex

: Baud rate: 9600/38400/115200 b/s

: Data: 8 bits (Start Bit: 1 bit; Stop Bit: 1 bit)

- IP Control	: Web API: HTTP

Power	: 100-230 VAC, 50/60 Hz

Power consumption	: < 30W

Dimensions (WxDxH)	: 430 x 43 x 200 mm

Weight	: 2.5kg

* DN-700CB 동급이상품