*) Omni Boundary Layer Mic

1. 개요

본 기기는 바운더리 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

The BLM4060 features a stainless steel base and rubber center which holds the capsule and effectively absorbs shock and vibration noise.

The frequency response is optimized for greater intelligibility of speech.

The hemispherical omnidirectional polar pattern effectively captures talkers seated around the microphone while rejecting reflections of the table surface.

The omnidirectional polar pattern provides a uniform frequency and sensitivity response at the perimeter of the capsule, allowing talkers to speak freely from any position in relationship to the microphone placement.

3. 규격 및 사양

Operating Principle	: Pressure Gradient

Transducer	: Condenser

Polar Pattern	: Omnidirectional

Frequency Range	: 20 Hz to 14 kHz

Signal-to-Noise Ratio	: 71 dB A-Weighted

Equivalent Noise Level	: 23 dB A-Weighted

: 35 dB ITU-R 468

Maximum SPL	: 134 dB SPL

THD	: < 1%

Sensitivity	: 20 mV/Pa

Dynamic Range	: 100 dB

Output Connectors	:1 x 3-Pin XLR

Operating Voltage	: 5 V

Operating Temperature	: 14 to 113°F / -10.00 to 45.00°C

Diameter	: 3.94" / 100 mm

Weight	: 8.5 oz / 241 g

Package Weight	: 1.15 lb

Box Dimensions (LxWxH)	: 8.75 x 5.3 x 1.65"

* 4060-OL-D-S01-001 동급이상품