*) PIN MIC

1. 개요

본 기기는 무선 바디팩 송신기에 연결하여 사용 할 수 있는 핀 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Exceptional audio quality

Uniform, consistent sound between DPA mics

Extremely rugged and reliable

Diminutive size made for flexible and easy concealment

Large selection of clips, windscreens, grids and other accessories

Modular adapter system fits most professional wireless systems

3. 규격 및 사양

Directional pattern	: Omnidirectional

Principle of operation	: Pressure

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range ±2 dB

Soft boost grid	: 20 Hz - 20 kHz, 3 dB soft boost at 8 – 20	kHz.

High boost grid	: 20 Hz- 20 kHz, 10 dB boost at 12 kHz

Sensitivity, nominal, ±3 dB at 1 kHz	: 6 mV/Pa; -44 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 26 dB(A) re. 20 μPa (max. 28 dB(A))

Equivalent noise level, ITU-R BS.468-4	: Typ. 38 dB (max. 40 dB)

Distortion, THD < 1% - CORE	: 134 dB SPL RMS, 137 dB SPL peak

Dynamic range - CORE	: Typ. 111 dB

Max. SPL, THD 10%	: 144 dB SPL peak

Rated output impedance	: 30 - 40 Ω

Cable drive capability	: Up to 300 m (984 ft) with DAD6001-BC XLR	Adapter

Power supply (for full performance)

For wireless systems	: Min. 5 V - max. 10 V through DPA adapter

With DAD6001-BC	: P48 (Phantom Power). Will work from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD6001-BC XLR Adapter

Connector	: MicroDot, TA4F Mini-XLR, 3-pin LEMO,	Mini-Jack

Color	: Black, beige, brown or white

Weight	: 7.5 g (0.26 oz) incl. Cable and MicroDot	connector

Microphone diameter	: 5.4 mm (0.21 in)

Microphone length	: 12.7 mm (0.5 in)

Cable length	: 1.8 m (5.9 ft)

Polarity	: Positively increasing sound pressure produces	positive going voltage on MicroDot pin

Temperature range	: -40°C to 45°C (-40°F to 113°F)

Relative humidity (RH)	: Up to 90%

Sensitivity selection tolerance (at 1kHz)	: ±1.5 dB

* 4061 동급이상품