*) PIN MIC

1. 개요

본 기기는 무선 바디팩 송신기에 연결하여 사용 할 수 있는 핀 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Excellent speech reproduction

Discreet, compact design

Fits both left and right buttoned shirts

Delivered with both black and white pop filters

Modular adapter system fits most professional wireless systems

3. 규격 및 사양

Directional pattern	: Cardioid

Principle of operation	: Pressure gradient

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range, ±2 dB, at 25 cm (9.8 in)	: 250 Hz - 17 kHz with typ. 4 dB soft boost at	4 - 6 kHz (-5 dB at 100 Hz)

Sensitivity, nominal, ±3 dB at 1 kHz	: 20 mV/Pa; -34 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 23 dB(A) re. 20 µPa (max. 26 dB(A))

Distortion, THD < 1% - CORE	: 126 dB SPL RMS, 129 dB SPL peak

Dynamic range	: Typ. 100 dB

Max. SPL, THD 10%	: 134 dB SPL peak

Rated output impedance	: 30 - 40 Ω

Cable drive capability	: Up to 300 m (984 ft) with DAD6001-BC XLR	Adapter

Power supply (for full performance)

For wireless systems	: Min. 5 V - max. 10 V through DPA adapter

With DAD6001-BC	: P48 (Phantom Power). Will work from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD6001-BC XLR Adapter

Connector	: MicroDot, TA4F Mini-XLR, 3-pin LEMO,	Mini-Jack

Color	: Black

Weight	: 15 g (0.5 oz) incl. Cable and MicroDot	connector

Microphone diameter	: 5.7 mm (0.22 in)

Microphone length	: 30 mm (1.2 in)

Cable length	: 1.2 m (3.9 ft)

Cable diameter	: 1.6 mm (0.06 in)

Polarity	: Positively increasing sound pressure produces	positive going voltage on MicroDot pin

Temperature range	: -40°C to 45°C (-40°F to 113°F)

Relative humidity (RH)	: Up to 90%

* 4080 동급이상품