*) GOOSENECK MICROPHONE

1. 개요

본 기기는 마이크의 방향을 자유롭게 움직일 수 있는 구즈넥 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Small footprint, lightweight

Enhances speech intelligibility

Built-in shock mount

Resistant to moisture, extreme temperatures and humidity

Extensions and range of mounting options available (4099 series of clips)

Specific interview kit for broadcast

3. 규격 및 사양

Directional pattern	: Supercardioid

Principle of operation	: Pressure gradient

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range ±2 dB, at 20 cm (7.9 in)	: 80 Hz - 15 kHz with 2 dB soft boost at 10-12	kHz

Sensitivity, nominal, ±3 dB at 1 kHz	: 16 mV/Pa; -36 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 23 dB(A) re. 20 µPa (max. 26 dB(A))

Equivalent noise level, ITU-R BS.468-4	: Typ. 35 dB (max. 38 dB)

Distortion, THD < 1%	: 130 dB SPL RMS, 133 dB SPL peak

Dynamic range	: Typ. 110 dB

Max. SPL, THD 10%	: 135 dB SPL peak

Rated output impedance

From MicroDot	: 30 - 40 Ω.

From DAD4099-BC XLR Adapter	: 100 Ω

Cable drive capability	: Up to 300 m (984 ft) with DAD4099-BC XLR	Adapter

Common mode rejection ratio (CMRR)	: > 60 dB from 50 Hz to 15 kHz with	DAD4099-BC XLR Adapter

Power supply (for full performance)

For wireless systems	: Min. 5 V - max. 10 V through DPA adapter

With DAD6001-BC	: P48 (Phantom Power). Will work from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD6001-BC XLR Adapter

Connector	: MicroDot

Color	: Black

Weight	: 10 g (0.35 oz)

Microphone length	: 10.4 cm (4 in)

Temperature range	: -40°C to 45°C (-40°F to 113°F)

Relative humidity (RH)	: Up to 90%

* 4097 동급이상품