*) PIN MIC

1. 개요

본 기기는 무선 바디팩 송신기에 연결하여 사용 할 수 있는 핀 마이크로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Amazing 3 mm CORE capsule technology

Renowned DPA sound in a 60% smaller package

Stainless steel, PVD-coated mic housing

Modular adapter system fits most professional wireless systems

3. 규격 및 사양

Directional pattern	: Omnidirectional

Principle of operation	: Pressure

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range ±2 dB	: 40 Hz - 20 kHz with 4 dB soft boost at 8 -	20 kHz

Sensitivity, nominal, ±3 dB at 1 kHz	: 20 mV/Pa; -34 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 24 dB(A) re. 20 μPa (max. 26 dB(A))

Distortion, THD < 1%	: 123 dB SPL RMS, 126 dB SPL peak

Dynamic range	: Typ. 102 dB

Max. SPL, THD 10%	: 134 dB SPL peak

Rated output impedance	: 30 - 40 Ω

Cable drive capability	: Up to 300 m (984 ft) with DAD6001-BC XLR	Adapter

Power supply (for full performance)

For wireless systems	: Min. 5 V - max. 10 V through DPA adapter

With DAD6001-BC	: P48 (Phantom Power). Will work from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD6001-BC XLR Adapter

Connector	: MicroDot, TA4F Mini-XLR, 3-pin LEMO,	Mini-Jack

Color	: Black, beige, brown or white

Weight	: 8 g (0.29 oz) incl. Cable and MicroDot	connector

Microphone head size (h x w x d)	: 3.4 / 14.4 mm (0.13 / 0.57 in)

Capsule diameter	: 3 mm (0.12 in)

Cable length	: 1.8 m (5.9 ft)

Polarity	: Positively increasing sound pressure produces	positive going voltage on MicroDot pin

Temperature range	: -40°C to 45°C (-40°F to 113°F)

Relative humidity (RH)	: Up to 90%

* 6060 동급이상품