*) CLASSIC TOURING MICROPHONE SET

1. 개요

본 기기는 악기용 투어링 마이크 세트로 다음과 같은 규격에 준한다.

2. 규격 및 사양

Directional pattern	: Supercardioid

Principle of operation	: Pressure gradient

Cartridge type	: Pre-polarized condenser

Frequency response	: 20 Hz - 20 kHz

Effective frequency range ±2 dB, at 20 cm (7.9 in)	: 80 Hz - 15 kHz with 2 dB soft boost	at 10-12 kHz

Sensitivity, nominal, ±3 dB at 1 kHz	: 6 mV/Pa; -44 dB re. 1 V/Pa

Equivalent noise level, A-weighted	: Typ. 23 dB(A) re. 20 μPa (max. 26 dB(A))

Distortion, THD < 1%	: 128 dB SPL RMS, 131 dB SPL peak

Dynamic range	: Typ. 108 dB

Max. SPL, THD 10%	: 142 dB SPL peak

Rated output impedance	: From MicroDot: 30 - 40 Ω. From DAD4099-BC	or DAD6001-BC: 100 Ω

Cable drive capability	: Up to 300 m (984 ft) with	DAD6001-BC/DAD4099-BC XLR Adapter

Output balance principle	: Signal balanced with DAD4099-BC or	DAD6001-BC XLR Adapter

Common mode rejection ratio (CMRR)	: > 60 dB from 50 Hz to 15 kHz with	DAD4099-BC or DAD6001-BC XLR Adapter

Power supply (for full performance)	: For wireless systems Min. 5 V - max. 10 V	through DPA adapter With DAD6001-BC or	DAD4099-BC: P48 (Phantom Power). Will work	from 12 V

Current consumption	: Typ. 1.5 mA (microphone). 3.5 mA with	DAD4099-BC or DAD6001-BC XLR Adapter

Connector	: MicroDot

Weight

- Microphone: 17 g (0.60 oz)

- Instrument Microphone Clamp Mount (CM4099): 16 g (0.56 oz)

- Instrument Microphone Clip for Accordion (AC4099): 5 g (0.18 oz)

- Instrument Microphone Clip for Bass (BC4099): 20 g (0.71 oz)

- Instrument Microphone Clip for Cello (CC4099): 13 g (0.46 oz)

- Instrument Microphone Clip for Drum (DC4099): 13 g (0.46 oz)

- Instrument Microphone Clip for Guitar (GC4099): 12 g (0.42 oz)

- Instrument Microphone Clip for Piano (PC4099): 19 g (0.67 oz)

- Instrument Microphone Clip for Sax and Trumpet (STC4099): 7 g (0.25 oz)

- Instrument Microphone Clip for Violin and Mandolin (VC4099): 10 g (0.35 oz)

- Universal Instrument Microphone Clip (UC4099): 15 g (0.53 oz)

- Mic Stand Mount for Instrument Microphone (MS4099): 28 g (0.99 oz)

- Cold Shoe Mount with standard 1/4" in thread (CS4099): 5 g (0.18 oz)

Microphone diameter	: 5.7 mm (0.22 in)

Microphone length	: 45 mm (1.8 in)

Cable length	: 1.8 m (5.9 ft)

Cable diameter	: 1.6 mm (0.06 in) / 2.2 mm (0.09 in)

Polarity	: +V at MicroDot pin for positive sound pressure	(and pin 2 on DAD4099-BC or DAD6001-BC	XLR adapter)

Temperature range	: -40°C to 45°C (-40°F to 113°F)

Relative humidity (RH)	: Up to 90%

Gooseneck length	: 140 mm (5.5 in)

Sensitivity selection tolerance (at 1 kHz)	: ±1 dB

Component

- 4099 Loud SPL 마이크 x 10EA

- 1.6mm 연장 케이블(길이:1.8m) x 10EA

- XLR어뎁터 x 10EA

- 스텐드 마운트 x 1EA

- 클램프 파운트 x 2EA

- 색소폰용 클립 x 2EA

- 피아노용 클립 x 2EA

- 베이스용 클립 x 2EA

- 첼로용 클립 x 2EA

- 기타용 클립 x 4EA

- 바이올린용 클립 x 8EA

- 유니버셜 클립 x 2EA

- 펠리칸 케이스 x 1EA

* KIT-4099-DC-10C 동급이상품