*) AES50 EXTENDER

1. 개요

본 기기는 네트워크 오디오 신호를 분배/전송 가능한 익스텐더로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Dual Port AES50 Extenders and 19" rackmount adapter bracket

Extends two AES50 connections by 500 m with optical fi bre or 100 m with Cat5 cable

High channel capacity - 48 channels@ 96 kHz or 96 channels @ 48 kHz bidirectional operation

Neutrik etherCON* connectors used for AES50 ports and copper snake connection

Dual-fi bre Neutrik opticalCON DUO connector used for optical fibre snake connection

Comprehensive clock source options with front panel push button selection and LED indication

Status indicator LEDs on front panel for each AES50 port and optical and copper snake connections

Rugged half-width 1U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

AES50

- Ports	: 2

- Type	: Neutrik etherCON with LED status indication

- Sample rate	: 48 kHz, 96 kHz

Copper

- Snake Port	: 1

- Type	: Neutrik etherCON

Optical Snake Port

- Snake Port	: 1

- Type	: Neutrik opticalCON DUO

- Optical fibre	: Multimode dual fibre

Clock Source

- Options	: Internal clock, External AES50 clock,	External snake clock

USB configuration port	: USB 2.0 Type B connector

Power Requirements

- Voltage	: 100 to 240 VAC, 50 to 60 Hz

- Consumption	: <50W

Dimensions (WxDxH)	: 217 x 263 x 44 mm

Weight	: 2.4 kg

* DN9620 동급이상품