*) SPLITTER

1. 개요

본 기기는 오디오 신호를 증폭하여 분배하는 장비로 다음과 같은 규격에 준한다.

2. 기능 및 특성

12 channel microphone splitter with 4 transformer balanced outputs per channel

Solo bus with integrated headphone amplifier and level control

Independent +30 dB and -15 dB gain switches per channel

+48 V phantom power switch and earth lift switch per channel

Input and Output 1 duplicated on front and rear panels for cable looming fl exibility

Individual LED metering for each channel

Rugged 3U rackmount chassis for durability in portable applications

Dual redundant auto-ranging universal switch-mode power supplies

3. 규격 및 사양

Inputs

Input impedance	: > 2 kΩ

CMRR	: > -100 dB @ 100 Hz to 10 kHz

Equivalent input noise	: < -100 dBu @ unity gain

Signal present level	: > -25 dBu

Signal clip level	: > +21 dBu

Transformer-balanced outputs

Source impedance	: 70 Ω

Min load	: 600 Ω (-3 dB level loss into 200 Ω )

Max level	: + 18 dBu @ 1 kHz

Connectors	: 3 pin male XLR (external),	3 way terminal strip (internal)

Frequency response	: +0 / -1.0 dB 20 Hz to 20 kHz

Distortion	: < 0.04% @ 1 kHz +4 dB

Audio Inputs / Outputs	: 3 pin XLR

Power	: IEC

Voltage	: 100 to 240V ± 10% 50/60 Hz <60W

Dimensions (WxDxH)	: 483 x 319 x 132 mm

Weight	: 7.4 kg

* DN1248PLS-FM 동급이상품