*) DSP POWER AMP

1. 개요

본 기기는 DSP를 내장한 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Dante 컨트롤러의 완벽한 지원

랩그루핀 고유의 전원효율 관리시스템(RPM)

앰프의 자원을 효율적으로 사용하기 위해 채널 전체에 걸쳐 요구되는 파워에 대응하여 출력 전력을 효율적으로 재할당하는 완전한 유연성 보장

4개 회로의 데이터 처리량을 제공하는 Lake 고유의 클래식/선형위상/FIR 스피커 프로세싱

그룹 컨트롤이 가능한 Raised Cosine™ MESA EQ™ 비대칭 필터

낮은 레이턴시(저지연)의 샘플레이트 변환이 가능한 포괄적인 디지털 클럭 관리시스템

AES3 디지털 입력 2개(오디오 채널 4개)

AES67을 지원하는 8개의 이중 이원화 Dante 네트워크 오디오 입력

입력신호에 장애 발생 시 차 순위 입력으로 순간 전환을 위한 프로그래밍이 가능한 다중 및 예비 입력

광범위한 종류의 스피커 프리셋 데이터베이스(LoadLibrary™)

3. 규격 및 사양

General

Processing / Network	: Lake / Dante

Number of amplifier channels	: 4

Total burst power all channels (share among channels with RPM)	: 12000 W

Max. Output Power (all ch.’s driven)

2 ohms	: 3000 W

2.67 ohms	: 3000 W

4 ohms	: 3000 W

8 ohms	: 1900 W

16 ohms	: 950 W

Hi-Z 70 V	: 3000 W

Hi-Z 100 V	: 3000 W

Max. Output power bridged mode (all ch.’s driven)

4 ohms	: 6000 W

8 ohms	: 6000 W

16 ohms	: 3800 W

Max output power single channel (all models)

2 ohms	: 4400 W

2.67 ohms	: 5900 W

4 ohms	: 4600 W

8 ohms	: 2300 W

16 ohms	: 1150 W

Hi-Z 70 V	: 3300 W

Hi-Z 100 V	: 4700 W

Audio Performance (Amplifier platform with digital input)

THD + N 20 Hz - 20 kHz for 1 W : < 0.05 %

THD + N at 1 kHz and 1 dB below clipping	: < 0.04 %

Dynamic range	: > 114 dB

Channel separation (Crosstalk) at 1 kHz	: > 70 dB

Frequency response (1 W into 8 ohm, 20 Hz - 20 kHz)	: +/- 0.05 dB

Internal sample rate / Data path	: 48 / 96 kHz / 32 bit floating point

Product propagation delay AES 96 kHz / analog input	: 1.61 / 1.68 ms

Dimensions (WxHxD)	: 483 (19”) x 88 (2 U) x 424 mm

Weight	: 15.8 kg

Finish	: Black painted steel chassis with grey painted	steel front with detachable grille

* D120:4L 동급이상품