*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Optimized for sustained performance into extreme low-frequency loads, yet it also maintains Lab.gruppen’s reputation for exceptionally smooth and transparent mid- and high-frequency response

Monitoring and control of key functions accessible via the intuitive DeviceControl software and the robust, daisy-chained NomadLink network, as well as by the leading third party control platforms

Road-proven output stage delivers Class B audio quality with Class D efficiency

Output power remains constant even with significant drops in the mains voltage

Unique, lightweight Intercooler® copper cooling system dissipates more heat to allow extended peak output

Selectable Gain, scalable Voltage Peak Limiter (VPL™), and bridge-mode operation allow custom configuration for any system or application

XLR input and link connectors

Heavy-duty binding posts

Excessive output current, DC, high temperature, very high frequency (VHF), short circuit, open load, mains fuse protection, and soft start

3. 규격 및 사양

General

Number of channels	: 2

Peak total output both channels driven	: 14000 W

Peak output voltage per channel	: 195 V

Max. output current per channel	: 90 A peak

Max. Output Power (Per ch. (both ch.’s driven) / Bridged per ch.)

2 ohms	: 7000 W / n.r.

4 ohms	: 4400 W / 14000 W

8 ohms	: 2350 W / 8800 W

16 ohms	: 1200 W / 4700 W

Performance with Gain: 35 dB and VPL: 195 V

THD 20 Hz - 20 kHz for 1 W	: <0.1%

THD at 1 kHz and 1 dB below clipping	: <0.05%

Signal To Noise Ratio	: >112 dBA

Channel separation (Crosstalk) at 1 kHz	: >70 dB

Frequency response (1 W into 8 ohms) +0/-3 dB	: 2 Hz - 34.2 kHz

Input impedance	: 20 kOhm

Common Mode Rejection (CMR)	: >54 dB, 20 Hz to 20 kHz

Output impedance @ 100 Hz	: 19 mOhm

Dimensions (WxHxD)	: 483 (19”) x 88 (2 U) x 396 mm

Weight	: 12 kg

Finish	: Black painted steel chassis with black painted	steel / aluminum front

* FP14000 동급이상품