*) POWER AMP

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하는 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

검증된 D클래스의 안정적인 앰프 출력단

고효율의 스위치모드 파워 서플라이(SMPS)

최대 출력레벨과 드라이버의 안정적인 보호를 위한 스피커 보호 리미터

로우컷, 하이컷 및 풀레인지 모드가 있는 통합 크로스오버

정밀한 전원 관리로 성능과 효율성을 동시에 보장

3. 규격 및 사양

General

Number of amplifier channels	: 2

Peak total output all channels driven	: 3000 W

Peak output voltage per channel	: 115 V

Peak output current per channel	: 32 A

Bridge mode	: No

Output circuit type	: Class-D

Amplifier Outputs

Max Output Power: All channels driven

- 2 Ω per channel, stereo	: 1000 W

- 4 Ω per channel, stereo	: 1500 W

- 8 Ω per channel, stereo	: 800 W

Audio Performance

THD+N 20 Hz - 20 kHz @ 1 W	: < 0.1%

THD+N @ 1kHz, 1 dB below clip	: < 0.1%

Signal-to-noise	: >90 dB

Channel separation (Crosstalk) @ 1 kHz	: >75 dB

Frequency response	: 10 Hz to 20 kHz, +0.5/ -1 dB

Input impedance	: 10 kΩ unbalanced, 20 kΩ balanced

Distortion,1/8 rated power	: < 0.1%

Dimensions (HxWxD)	: 93 x 483 x 326 mm

Weight	: 6.5 kg

Finish	: Black painted aluminium chassis and	grey front

* PD3000 동급이상품