*) DIGITAL AUDIO MIXING CONSOLE

1. 개요

본 기기는 디지털 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Graviton Audio Engine 내장

144 입력 및 120 버스 출력

96 stereo Effects

96 Ultima Stereo Dynamic EQs

32 Ultima Stereo Multiband Compressors

24 VCA (variable control association) groups, and 24 POPulation groups

21인치 풀컬러 TFT 고휘도 디스플레이 화면 (정전식 터치 감지 기능 탑재)

고도의 멀티 제스처 터치스크린 사용자 인터페이스

Midas 마이크 프리앰프

HyperMAC 및 AES50 네트워킹을 통해 최대 576개의 입력 및 576개의 출력 소스를 96kHz 샘플링 레이트로 사용

최대 128개의 양방향 채널과 비동기 샘플링 레이트 변환을 갖춘 듀얼 네트워크 브리지 형식 컨버터

내장 블루투스 및 무선 트랜시버 모듈

듀얼 ULTANET 포트 (32개의 디지털 출력을 추가 가능)

Midas PRO 모터식 100mm 페이더 28개

이중 리던던츠 자동 유니버셜 스위치 모드 전원 장치

TC electroic System 6000, 3000 , 2290 등 다양한 아웃보드 지원

3. 규격 및 사양

Processing

Input processing channels	: 144 flexi channels

Output processing channels	: 96 flexi aux outputs, 24 matrices, stereo bus,	mono bus

Internal effects engines	: 24 x effects slots (up to 96 effects)

: 32 x Stereo multiband compressors

: 96 x Stereo dynamic equalisers

Point-to-point routing matrix	: 622 x 652

Signal processing	: 64-bit floating point

D/A converter	: 24-bit, 96 kHz and 128 times oversampling

A/D converter	: 24-bit, 96 kHz and 128 times oversampling

Sampling frequency	: 96 kHz

I/O latency (surface input to output)	: 1.34 ms

Input audio processing	: Dual-slope high and low-pass filters

: True phase filter control

: 4-band parametric EQ with 3 shelf modes

: 4-mode creative input compressors

: Input gates or ducker

: Insert point on/off with processing order	change

: Direct output with adjustable level and	processing pick of point

: Delay-compensated aux return mode on inputs

: 5 x tap-off points per send

Output audio processing	: Output 4-band parametric EQ with	shelving/HP/LP options

: 4-mode creative output dynamics

: Insert point on/off with processing order	change

: Direct input with adjustable level and	processing tap-off point

Mixing control assistance	: 12 x talk groups

: 12 x mute groups

: 24 x surface POPulation groups

: 24 x VCA associated population groups

: Scene snapshot automation

Displays

Display screen	: 21" LCD high brightness 1920 x 1080 px,	captive touchscreen, up to 10 simultaneous	touches

LCD info displays	: 41 x full colour LCD info displays, 24 mm x 24	mm (size), 240 x 240 px

Controls

100 mm motorized faders	: 8 + 8 + 8 + 4

Touch-sensitive rotary controls	: 66

Fully assignable rotary controls	: 28 + 8

Fully assignable backlit buttons	: 28 + 8 + 12

Wi-Fi

Antenna	: Internal dual-band

IEEE 802.11 a/b/g/n	: Supports a / b / g / n devices

Frequency range	: 2412-2462 MHz / 5.15–5.850 GHz operation	dependent on region

Max output power	: 20 dBm (using 5 GHz range)

Bluetooth

Version	: 4.0 EDR and LE

Power	: 20 dBm

Compatibility	: Supports GAP, SDN, PAN, SPP, IAP, HFP 1.5,	GATT, ATTR, IAP, A2DP, ACRP.

Maximum communcation range	: 30 m typical

Power

Switch-mode power supply	: 2 x auto-ranging 100-240 V (50/60 Hz)

Power consumption	: 2 x 650 W

Current	: 9 A max

Physical

Dimensions (H x W x D)	: 352 x 1028 x 719 mm

Weight	: 43.2 kg

* HERITAGE-D 동급이상품