*) FIXED I/O BOX

1. 개요

본 기기는 Main Digital Mixer와 연동하여 사용가능한 Stage Box이다.

2. 기능 및 특성

16 award-winning MIDAS PRO microphone preamplifiers with switchable 48 V phantom power

8 electronically balanced low impedance line level outputs

ULTRANET personal monitoring system connectivity for in-ear applications

Digital audio and control connectivity for TURBOSOUND speaker systems with ULTRANET networking capability

Dual AES50 SuperMAC ports for cascading additional DL16 stageboxes—no merger or router required

Dual ADAT outputs providing 16-channel digital output on two optical TOSLINK* connectors

Remote operation via shielded CAT5e cable up to 330 ft / 100 m length

All settings programmable from front panel controls or console

Status indicator LEDs on front panel

Headphones output assignable to any of the inputs or outputs for on-stage monitoring

MIDI In/Out for bidirectional communication between MIDAS M32 Series console and on-stage MIDI devices

Features Neutrik etherCON* AES50 and ULTRANET network ports

Rugged 2U rackmount chassis for durability in portable applications

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Processing

A/D converters (8-channel, 24-bit @ 44.1 / 48 kHz)	: 114 dB dynamic range (A-weighted)

D/A converters (stereo, 24-bit @ 44.1 / 48 kHz)	: 120 dB dynamic range (A-weighted)

Networked I/O latency (stagebox in > console processing > stagebox out)	: 1.1 ms

Connectors

XLR inputs, programmable mic preamps	: 16

XLR outputs	: 8

Phones outputs, 1/4" TRS	: 1 (mono)

AES50 ports, SuperMAC, NEUTRIK etherCON	: 2

P-16 connector, Ultranet (no power supplied)	: 1

MIDI inputs / outputs	: 1 / 1

ADAT Toslink outputs (2 x 8 Ch)	: 2

USB type B, rear panel, for system updates	: 1

Power

Switch-mode autorange power supply	: 100-240 V (50/60 Hz)

Power consumption	: 45 W

Physical

Dimensions	: 482 x 225 x 89 mm

Weight	: 4.7 kg

* DL16 동급이상품.