*) ACTIVE HIGH OUTPUT TWO-WAY SPEAKER

1. 개요

본 기기는 앰프내장형 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1100 W Class D Amplifier

90 x 60 constant directivity coverage angle

15" neo woofer, 3.5" voice coil

1.5 " neo c. driver, 4.0" voice coil

DSP Processing

Onboard RDNet Control

Multifunctional cabinet

Very high output

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 50 Hz ~ 20000 Hz

Max SPL @ 1m	: 134 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 60°

Transducers

Compression Driver	: 1 x 1.5" neo, 4.0" v.c

Woofer	: 1 x 15" neo, 3.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 750 Hz

Protections	: Thermal, HF

Limiter	: Fast Limiter

Controls	: Proces., 8 sel. presets

RDNet	: Onboard

Power section

Total Power	: 2200 W Peak, 1100 W RMS

High frequencies	: 600 W Peak, 300 W RMS

Low frequencies	: 1600 W Peak, 800 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 6xfly track, quick lock, pole mount

Handles	: 2 on side

Grille	: Steel

Color	: Black

Size

Height	: 670 mm / 26.38 inches

Width	: 425 mm / 16.73 inches

Depth	: 425 mm / 16.73 inches

Weight	: 26 kg / 57.32 lbs

* TT 25-A II 동급이상품