*) ACTIVE FLYABLE SUBWOOFER MODULE

1. 개요

본 기기는 라인 어레이 형태로 설치 가능한 앰프내장형 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

136 dB Max SPL

3200W peak class-D Amplifier

30~140 Hz frequency response

RDNet Networked Management

1x18” Neodymium Woofer, 4.0” voice coil

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 30 Hz ~ 140 Hz

Max SPL @ 1m	: 136 dB

Transducers

Woofer	: 1 x 18" neo, 4.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: +4 dBu

Processor section

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, Preset selection

RDNet	: Onboard

Power section

Total Power	: 3200 W Peak, 1600 W RMS

Low frequencies	: 3200 W Peak, 1600 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Array fittings, 1 X M20

Handles	: 2 Side

Pole mount/Cap	: M20 thread

Grille	: Steel

Color	: Black, White - RAL 9003

Size

Height	: 502 mm / 19.76 inches

Width	: 700 mm / 27.56 inches

Depth	: 621 mm / 24.45 inches

Weight	: 48.7 kg / 107.36 lbs

* HDL 38-AS 동급이상품