*) ACTIVE HIGH POWER SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

2500 Watt Peak

136 dB max SPL

30 Hz - 120 Hz frequency response

18" Woofer, 4.0" voice coil vented woofer

DSP controlled Input section with selectable presets

Delay control

Baltic birch tour grade cabinet

Compatible with NXL23-A (stacking)

Compatible with NXL24-A (stacking)

Multiple configurations with HDL 10-A and HDL 20-A

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 30 Hz ~ 120 Hz

Max SPL @ 1m	: 136 dB

Transducers

Woofer	: 1 x 18", 4.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR

Output connectors	: XLR

Input sensitivity	: -2 dBu / +4 dBu

Processor section

Hi-Pass Frequencies	: 120 Hz

Low-Pass Frequencies	: 90 Hz

Protections	: Thermal, RMS

Limiter	: Fast Limiter

Controls	: Xover, Phase switch, Deep/Punch, Outuput	Delay Settings, Cardioid

Power section

Total Power	: 2500 W Peak, 1250 W RMS

Low frequencies	: 2500 W Peak, 1250 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Pole mount/Cap	: M20 thread

Color	: Black

Physical specifications

Height	: 700 mm / 27.56 inches

Width	: 558 mm / 21.97 inches

Depth	: 700 mm / 27.56 inches

Weight	: 56 kg / 123.46 lbs

* SUB 8004-AS 동급이상품