*) PROFESSIONAL POWERED DUAL 18" SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 앰프내장형 제품이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 137 dB Sound Pressure Level

4400W Class-D Bi-Amplification

30-120 Hz linear frequency response

2 x 18" High Power Woofers

IP Rated Powercon TRUE1 TOP IN/OUT

8 Crossover Presets and 4 Cardioid Presets

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 30 Hz ~ 120 Hz

Max SPL @ 1m	: 137 dB

Transducers

Woofer	: 2 x 18", 4.0" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR

Output connectors	: XLR

Input sensitivity	: -2 dBu / +4 dBu

Processor section

Crossover Frequencies	: Selectable

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Xover, Phase switch, Deep/Punch, Outuput	Delay Settings

Power section

Total Power	: 4400 W Peak

Low frequencies	: 4400 W Peak

Cooling	: Convection/Forced

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 2 x M20

Handles	: 2 x side

Pole mount/Cap	: M20 thread

Grille	: Steel

Color	: Black

Physical specifications

Height	: 550 mm / 21.65 inches

Width	: 1180 mm / 46.46 inches

Depth	: 700 mm / 27.56 inches

Weight	: 80 kg / 176.37 lbs

* SUB 8008-AS 동급이상품