*) PROFESSIONAL ACTIVE SPEAKER

1. 개요

본 기기는 앰프내장형 포인트소스 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 130 dB Sound Pressure Level

2100W Class-D Bi-Amplification

50-20000 Hz linear frequency response

1.75" Compression Driver

12" Woofer

FiRPHASE zero degrees phase technology

Bass Motion Control woofer excursion management

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 50 Hz ~ 20000 Hz

Max SPL @ 1m	: 130 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 60°

Transducers

Compression Driver	: 1 x 1.0", 1.75" v.c

Woofer	: 1 x 12", 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 1600 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Linear, Boost, Stage, Volume

Power section

Total Power	: 2100 W Peak

High frequencies	: 700 W Peak

Low frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: VDE

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 2 x M10 Top, 1 x M10 each side,	1 x M10 bottom, 1 x M10 rear

Handles	: 1 x Side

Pole mount/Cap	: 35 mm insert

Grille	: Steel

Color	: Black

Size / Weight

Height	: 620 mm / 24.41 inches

Width	: 362 mm / 14.25 inches

Depth	: 405 mm / 15.94 inches

Weight	: 20.8 kg / 45.86 lbs

* NX 912-A 동급이상품