*) ACTIVE TWO-WAY ARRAY

1. 개요

본 기기는 앰프내장형 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1,400 WATT Class D Bi-Amplification

90° x 30° constant directivity waveguide, tilted (+5°, -25°)

3 x 10" neodymium woofer

1.4" compression neodymium driver, 3.0" voice coil

DSP Processing with optimized phase response

Easy-to-fly and install with built-in rigging points

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 45 Hz ~ 20000 Hz

Max SPL @ 1m	: 134 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 30°

Transducers

Compression Driver	: 1 x 1.4" neo, 3.0" v.c

Woofer	: 3 x 10" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 800 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, EQ Shape, Mic/Line

Power section

Total Power	: 1400 W Peak, 700 W RMS

High frequencies	: 400 W Peak, 200 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 4 x M8, 4 x quick lock, 2 x pole mount

Handles	: 4 side

Pole mount/Cap	: Yes

Grille	: Steel

Color	: Black

Size

Height	: 1198 mm / 47.17 inches

Width	: 303 mm / 11.93 inches

Depth	: 402 mm / 15.83 inches

Weight	: 34.5 kg / 76.06 lbs

* NXL 44-A 동급이상품