*) ACTIVE TWO-WAY ARRAY

1. 개요

본 기기는 앰프내장형 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1,400 Watt Class D bi-amplification

131 dB SPL Max

65 Hz ~ 20 kHz frequency response

4 x 6" Woofers

2.5" voice coil RCF Precision C. Driver on a waveguide

100° x 30° slightly tilted pattern control

DSP controlled input section with single or dual EQ preset

East-to-fly and install with built-in rigging points and pole mount socket

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 65 Hz ~ 20000 Hz

Max SPL @ 1m	: 131 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 30°

Transducers

Compression Driver	: 1 x 1.4", 2.5" v.c

Woofer	: 4 x 6.0", 1.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 800 Hz

Protections	: Thermal, RMS

Limiter	: Soft Limiter

Controls	: Volume, EQ Shape, MIc/Line

Power section

Total Power	: 1400 W Peak, 700 W RMS

Low frequencies	: 1000 W Peak, 500 W RMS

Cooling	: Convection

Connections	: Powercon IN/OUT

Physical specifications

Dimensions	: W 1056 x H 201 x D 274 mm

Weight	: 26.4kg

Color	: Black

* NXL 24-A 동급이상품