*) ACTIVE TWO-WAY ARRAY

1. 개요

본 기기는 앰프내장형 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 135 dB Sound Pressure Level

2100W Class-D Amplifier

100° x 50° Constant Directivity Coverage Angle

3" Titanium Neodymium Compression Driver

3 x 10" High Power Neodymium Woofers

45-20000 Hz linear Frequency Response

Bass Motion Control and FiRPHASE processing

8 x M8 Rigging Points and 8 x Quick Lock

IP Rated Powercon TRUE1 TOP IN/OUT

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 45 Hz ~ 20000 Hz

Max SPL @ 1m	: 135 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 50°

Transducers

Compression Driver	: 1 x 1.4" neo, 3.0" v.c

Woofer	: 3 x 10" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: Combo XLR, Jack

Output connectors	: XLR

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 800 Hz

Protections	: Thermal, Excurs., RMS

Limiter	: Soft Limiter

Controls	: Linear, Boost, High-Pass presets, Volume

Power section

Total Power	: 2100 W Peak

High frequencies	: 700 W Peak

Low frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 8 x M8, 8 x quick lock

Handles	: 2 side

Pole mount/Cap	: Yes

Grille	: Steel

Color	: Black

Size

Height	: 1080 mm / 42.52 inches

Width	: 297.5 mm / 11.71 inches

Depth	: 377 mm / 14.69 inches

Weight	: 31.55 kg / 69.56 lbs

* NXW 44-A 동급이상품