*) TWO-WAY PROFESSIONAL SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

300 W RMS power handling

128 dB max SPL

60 ~ 20000 Hz frequency range

90° x 70° constant directivity coverage angle

1 x 10" high power woofer

1 x 1.4" voice coil compression driver

High quality plywood cabinet

Steel front grille with clothing

Installation points available on rear, top and bottom panels

4 pole EUROBLOCK connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 128 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 70°

Directivity index Q	: 9

System Sensitivity	: 98 dB

Power section

Nominal Impedance (ohm)	: 8 ohm

Power Handling	: 300 W RMS

Peak Power Handling	: 1200 W PEAK

Recommended Amplifier	: 600 W

Protections	: Dynamic active mosfet

Crossover Frequencies	: 1800 Hz

Transducers

Compression Driver	: 1x1.0", 1.4" v.c

Nominal Impedance	: 8 ohm

Input Power Rating	: 25 W AES, 50 W PROGRAM POWER

Sensitivity	: 107 dB, 1W @ 1m

Woofer	: 10", 2.5" v.c

Nominal Impedance	: 8 ohm

Input Power Rating	: 300 W AES, 600 W PROGRAM POWER

Sensitivity	: 98 dB, 1W @ 1m

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 8 x M8, 8 x M10

Grille	: Steel with clothing

Color	: Black - RAL 9005, White - RAL 9003

Size

Height	: 510 mm / 20.08 inches

Width	: 295 mm / 11.61 inches

Depth	: 325 mm / 12.8 inches

Weight	: 17 kg / 37.48 lbs

* COMPACT M 10 동급이상품