*) HORN LOADED TWO-WAY ARRAY 60° X 22.5°

1. 개요

본 기기는 방수 기능을 갖춘 중/장거리용 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1500 W system power handling (RMS)

141 dB max SPL

60° x 22.5° constant directivity, horn-loaded

IP 55 protection code

60 Hz ~ 20000 Hz frequency range

2 x 12" high power woofers (3.5" v.c.)

1 x 4.0" v.c. compression driver, titanium dome

Baltic Birch Plywood enclosure with internal structural metal bracings

Safe and solid variable array mechanics

Amphenol IP 67 in/out connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Frequency Response (-3dB)	: 80 Hz ~ 20000 Hz

Max SPL @ 1m	: 141 dB

Horizontal coverage angle	: 60°

Vertical coverage angle	: 22.5°

Directivity index Q	: 14

Power section

Amplification	: Bi-Amp

Crossover Frequencies	: 600 Hz

Nominal Impedance LF	: 8 ohm

Power Handling LF	: 1350 W

Peak Power Handling LF	: 5400 W

Sensitivity LF	: 104 dB

Nominal Impedance HF	: 8 ohm

Power Handling HF	: 150 W

Peak Power Handling HF	: 600 W

Sensitivity HF	: 113 dB

Transducers

Compression Driver	: 1 x 2.0" neo, 4.0" v.c

Woofer	: 2 x 12", 3.5" v.c

Input/Output section

Input connectors	: Amphenol eco/mat IP 67

Output connectors	: Amphenol eco/mat IP 67

Standard compliance

IP protection grade	: IP 55

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: Side and rear array rigging point

Grille	: Steel

Color	: Black

Size

Height	: 530 mm / 20.87 inches

Width	: 771 mm / 30.35 inches

Depth	: 635 mm / 25 inches

Weight	: 66 kg / 145.5 lbs

* HL 2260 동급이상품