*) 4 INPUTS, 8 OUTPUT DIGITAL PROCESSOR

1. 개요

본 기기는 스피커 시스템을 제어하기 위한 디지털 프로세서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

The DX 4008 is a complete 4 input - 8 output digital loudspeaker management system designed for the touring or fixed sound installation markets

Sampling rate can be set to 96kHz

Precise frequency control is achieved with its 1 Hz resolution

Inputs and outputs can be routed in multiple configuration to meet any requirements

The DX 4008 is shipped with a special PC Graphic User Interface (GUI) application - XLink

XLink gives the user an option to control the DX 4008 unit from a remote PC via the RS232 serial communication link

The GUI application makes much easier control and monitor the device, allowing the user to get the whole picture on one screen

Programs can be recalled and stored from/to PC's hard drive, thus expanding the storage to become virtuality limitless

3. 규격 및 사양

Audio performance

Frequency Response (-3dB)	: 20 Hz ~ 20 kHz

Crosstalk (on the whole bandwitch)	: <-100 dB

Distortion (THD+N) @ 1 kHz nominal power	: <0.001 %

Dynamic range	: >115 dB

Common Mode Rejection Ratio (50 Hz to 10 kHz)	: >60 dB

Digital audio performance

Resolution	: 40

Sampling rate	: 96

A/D - D/A converters	: 24

Propagation delay	: 3

Input section

Total number of inputs	: 4

Balanced	: 4

Mono	: 4

Line inputs	: 4

Line connectors	: XLR

Output section

Signal output number	: 8

Signal output connectors	: XLR

Processing

DSP	: Yes

EQ Filters	: Yes

Delay	: Yes

Tone controls	: Yes

High-pass filter	: 20 Hz ~ 20000 Hz

Crossover	: 20 ~ 20000 Hz

Controls

Configuration	: Front panel, PC Software

Number of programs/presets	: 30

Protocols for system integration	: ASCII

Protections

Cooling	: Convection

Fuses	: Yes

Power requirement

Operating voltage	: 220-240/115 V~ 50/60Hz

Voltage selection	: External

Power consumption	: 20 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Color	: Black

Rack mounting	: 19", 1U

Size

Height	: 44 mm / 1.73 inches

Width	: 483 mm / 19.02 inches

Depth	: 203 mm / 7.99 inches

Weight	: 2.96 kg / 6.53 lbs

* DX 4008 동급이상품