*) 16-CHANNEL MIXING CONSOLE WITH MULTI-FX & RECORDING

1. 개요

본 기기는 아날로그 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

10 Mic preamp inputs, 4 mono line inputs

4 Stereo line inputs

PRO DSP FX onboard with 16 presets

Stereo recording and playback via USB port

6 single control compressors

Balanced main output +28 dB (Stereo XLR + TRS)

Two stereo output busses and 4 aux sends (2 pre, 1 pre/post, 1 post)

60 mm faders

Internal universal power supply

Designed and engineered in Italy

3. 규격 및 사양

Electronic specifications

Frequency Response	: 20 Hz ~ 20 kHz

THD+N, 20dB gain, 0dBu out	: <0,02% A-Weighted

Processing

Dynamic Range	: > 85dB

Inputs

Channels	: 16

Mic	: 10

Gain Range	: 0 dB ~ -50 dB

Input Noise Level	: -124 dBu A-Weighted

Mic Inputs Impedance	: 14 kohm

Low Cut	: 80 Hz

Phantom Power +48V	: Yes

Mono Line	: 8

Gain Selection	: 20 dB ~ -30 dB

Line Input Impedance	: 21 kohm

HI-Z Line Inputs	: 1

HI-Z Line Inputs Impedance (Mohm): 1 Mohm

Stereo Line	: 4

Gain Selection	: 20 dB ~ -30 dB

Stereo Line Input Impedance (kOhm): 14 kohm

Input Connectors	: XLR, Jack, RCA

Outputs

Main MIX	: 1

Control Room	: Yes

FX Send	: 1

AUX Send	: 3

AUX Output	: 4

Group Out	: 4

Phones	: 1

Output Connectors	: XLR, Jack

Outputs specifications

Main Out Level	: 28 dBu

Aux Out Level	: 28 dBu

Group Out Level	: 28 dBu

Phones Out impedance (ohm)	: 150 ohm

Phones Out Level	: 10 dBm

Compressors

RCF Compressors	: n°6 Single Control Compressors on	Channels 1 to 6

EQ

Input Channels EQ	: 1 Semi Parametric / 2 Shelving

Description	: High: +/-15 dB @ 10 kHz Shelving	Mid: +/-15 dB @ Freq. sel. from 100Hz to 8kHz	- Bell	Low: +/-15 dB @ 100 Hz Shelving

Auxiliary sends

AUX	: 2 PRE / 1 PRE/POST

FX POST	: 1

Internal Effects

Send Effects	: 1

USB audio

USB Audio Interface	: Yes

Type	: B

Play trk	: 2

Rec trk	: 2

Supported Sample Rate	: 44.1, 48.0 kHz

Other features

Footswitch	: Yes

Electrical specifications

Power supply	: Internal

Voltage requirements	: 100 V - 240 V

Power consumption (MAX)	: 30 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Color	: Black

Size

Height	: 107 mm / 4.21 inches

Width	: 479 mm / 18.86 inches

Depth	: 406 mm / 15.98 inches

Weight	: 6.4 kg / 14.11 lbs

* F 16XR 동급이상품