*) 6-CHANNEL MIXING CONSOLE WITH MULTI-FX

1. 개요

본 기기는 아날로그 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 Mic/Line inputs

2 stereo line inputs

One Aux/FX (post)

Balanced main output audio path from input to output

16 presets PRO DSP internal FX

Sturdy metal chassis

External universal power supply

Designed and engineered in Italy

3. 규격 및 사양

Electronic specifications

Frequency Response	: 20 Hz ~ 20 kHz

THD+N, 20dB gain, 0dBu out	: <0,02% A-Weighted

Processing

Dynamic Range	: > 85dB

Inputs

Channels	: 6

Mic	: 2

Gain Range	: 0 dB ~ -50 dB

Input Noise Level	: -124 dBu A-Weighted

Mic Inputs Impedance	: 14 kohm

Low Cut	: 80 Hz

Phantom Power +48V	: Yes

Mono Line	: 2

Gain Selection	: 20 dB ~ -30 dB

Line Input Impedance	: 21 kohm

Stereo Line	: 2

Gain Selection	: 20 dB ~ -30 dB

Stereo Line Input Impedance (kOhm): 15 kohm

Input Connectors	: XLR, Jack, RCA

Outputs

Main MIX	: 1

FX Send	: 1

AUX Output	: 1

Phones	: 1

Output Connectors	: XLR, Jack

Outputs specifications

Main Out Level	: 28 dBu

Aux Out Level	: 28 dBu

Phones Out impedance (ohm)	: 150 ohm

EQ

Input Channels EQ	: 2 Shelving / 1 Generic

Description	: High: +/-15 dB @ 10 kHz Shelving	Mid: +/-15 dB @ 1,250 kHz Bell	Low: +/-15 dB @ 100 Hz Shelving

Auxiliary sends

FX POST	: 1

Internal Effects

Send Effects	: 1

Other features

Footswitch	: Yes

Electrical specifications

Power supply	: External

Voltage requirements	: 100 V - 240 V

Power consumption (MAX)	: 12 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Color	: Black

Size

Height	: 79 mm / 3.11 inches

Width	: 210 mm / 8.27 inches

Depth	: 255 mm / 10.04 inches

Weight	: 1.8 kg / 3.97 lbs

* F 6X 동급이상품