*) GARDEN SPEAKER

1. 개요

본 기기는 목재, 콘크리트 등 여러 종류의 지면에 설치 가능하여 정원 등 야외 설치에 적합한 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Body made of linear low-density polyethylene

Coaxial transducer with 5,25"oofer and 1,20'' tweeter

Suitable for installation on different surfaces

Can be used in constant voltage lines 100V / 70V or in low impedance (8 ohm)

Protection grade IP56

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 111 dB

System Sensitivity	: 90 dB

Power section

Nominal Impedance	: 8 ohm

Power Handling	: 60 W RMS

Peak Power Handling	: 240 W PEAK

Recommended Amplifier	: 120 W

Transducers

Dome Tweeter	: 1 x 1.3"

Woofer	: 1 x 5.5"

Input/Output section

Constant Voltage Transformer	: 70/100 V

Power selection 1	: 32 W - 313 ohm

Power selection 2	: 16 W - 625 ohm

Power selection 3	: 8 W - 1250 ohm

Power selection 4	: 4 W - 2500 ohm

Power selection 5	: 2 W - 5000 ohm

Power selection 6 (100 V)	: 1 W - 10000 ohm

Standard compliance

IP protection grade	: IP 56

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PE Low Density

Color	: Green

Size

Height	: 409 mm / 16.1 inches

Diameter	: 365 mm / 14.37 inches

* GS 60 동급이상품