*) MULTIPAIR AES/EBU DMX & POWER COMBI CABLE

1. 개요

본 제품은 멀티 콤비 케이블로 다음과 같은 규격에 준한다.

2. 기능 및 특성

전원선과 DMX 신호를 하나의 케이블에 사용하여 조명기기의 병행 컨트롤

면과 비스코스로 만들어진 원형의 외피로 인해 매우 유연하고 내구성이 강함

촘촘한 나선형의 구리 메쉬 스크린과 꼬은 형태의 동으로 인해 DMX 라인과 한 쌍의 아주 좋은 차폐 효과

적용: DMX 조명 콘솔을 위한 컨트롤 선(웨이브 임피던스 110Ω), 전원 공급과 함께 아날로그 디지털 오디오 멀티채널 제공 등

3. 규격 및 사양

Properties	: OFC oxygen free copper

Signal transmission	: symmetrical

Construction	: [(3LIY1,5mm²)Y+	1x(2LI2Y0,25mm²)CY]VLY

Construction (power)	: (3LIY1,5mm²)Y

Construction (AES/EBU, DMX)	: 1x(2LI2Y0.25mm²)CY

Jacket material	: PVC

Jacket Ø [mm]	: 13,00

Jacket Ø (power) [mm]	: 6,20

Jacket Ø (AES/EBU, DMX) [mm]	: 4,00

Number of Channels (power)	: 1

Number of Channels (AES/EBU, DMX)	: 1

Inner conductor (power)	: 3

Inner conductor (AES/EBU, DMX)	: 2

Inner conductor (power) [mm²]	: 1,50

Inner conductor (AES/EBU, DMX) [mm²]	: 0,25

Inner conductor Ø (power) [mm]	: 1,38

Inner conductor Ø (AES/EBU, DMX) [mm]	: 0,56

AWG (power)	: 15

AWG (AES/EBU, DMX)	: 23

Shielding (AES/EBU, DMX)	: Braided mesh, tin-plated

Shielding factor [%]	: 85

Copper strands (power)	: 48

Copper strands (AES/EBU, DMX)	: 14

Copper strand Ø (power) [mm]	: 0,20

Copper strand Ø (AES/EBU, DMX) [mm]	: 0,15

Wire insulation material (power)	: PVC

Conductor insulation Ø [mm]	: 0,00

Conductor insulation Ø (power) [mm]	: 2,30

Conductor insulation Ø (AES/EBU, DMX) [mm]:1,25

Weight per 1 m [g]	: 200

UV-resistant	: yes

Fire load per m [kWh]	: 0,64

Style variant	: round

Packing	: bulk stock

Temperature min. [°C]	: -30

Temperature max. [°C]	: 70

Width [mm]	: 13

Height [mm]	: 13

* MONOLITH 1 동급이상품