*) 4K DECODER

1. 개요

본 기기는 네트워크 신호를 통해 비디오, 오디오 신호를 전송 할 수 있는 장비이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

A single Gigabit LAN Port for PoE Power, 4K60 4:4:4 Video, Dante™/AES67, and Control

Secure Network Isolation - VLAN Tagging separates AV traffic on the corporate network

One LAN drop to decoder enables local IP control of connected devices through Ethernet expansion port

Built in connectivity for web conference soft-codec AV integration

Eliminates need for separate AV Bridging hardware

Capture, record, and stream meetings directly to PC (USB-C)

Effortlessly share media from your USB-C enabled devices

Acts as an in-rack or Bring Your Own Device (BYOD) endpoint for presentation sharing and conferencing applications

Local input switching

Easy Control Integration

Ultra-low Latency [Sub-frame ~2ms visually lossless ]

Low bitrates

No fiber or 10 Gigabit switch required

Low-Cost network switches are used

Scalable / Unlimited Distribution

Any number and combination of inputs/outputs [in increments of one]

Standard network cabling [CAT5e/6]

Utilize existing network resources

Rapid deployment

Single network for AV and IT

Reduced operating costs

3. 규격 및 사양

Video Codec	: JPEG2000 based visually lossless video	compression algorithm

Audio Codec	: DANTE® / AES67

Bit Rates	: 50 to 800 Mbps

Latency

- Ultra-low Latency Sub-Frame (visually lossless video)

- ~2ms @ 1080p60 & 4K60 4:4:4

- ~4ms @ 1080p30 & 4K30

Streaming Protocols	: IP, UDP, TCP, ICMP, IGMP

Copy Protection	: HDCP 2.2, 2.3 AES-256 Encryption

Video

- Output	: 1x HDMI capable of scaling and outputting	video formats up to 4K60 4:4:4

: 1x USB-C capable of scaling and outputting	video formats up to 1080p60 4:4:4

Audio

- Output	: 1 digital audio output via HDMI

: 1 Analog Stereo Audio balanced output

: 1 Dante/AES67 digital audio output (up to 4ch)

Ethernet	: Network connectivity for control and IP traffic	pass-through to remote LAN devices

USB	: USB 2.0 host or device signal extension and	routing

GPIO	: For extension and control of third-party	devices

Serial / RS-232	: Bi-directional device control and monitoring

IR	: Device control via infrared

HDMI	: HDCP 2.2,2.3, CEC

Connectors

- LAN1	: 8-pin RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet port / PD port	: POE+ (IEEE 802.3at), POE+ Only required for	LAN2 PSE

- LAN2	: 8-pin RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet port / PSE port	: POE (IEEE 802.3af)

- HDMI OUTPUT	: HDMI Type A connector, female; HDMI digital	video/audio inputs

- USB-C OUTPUT	: (1) USB Type C connector, female;

- 1st - 8 pin Euroblock 3.81mm pitch connector	: Stereo Balanced Analog Audio Output

- 2nd - 8 pin Euroblock 3.81mm pitch connector	: Shared GPIO / RS-232 / IR ports

- USB Host	: (2) USB Type-A connector

Dimensions	(WxHxD)	: 146 x 28 x 230 mm

Weight	: 0.45 kg

* DuetD-5 동급이상품