*) Matrix Combiner

1. 개요

본 기기는 프로그래밍 가능한 다이버시티 매트릭스 결합기로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Combiner mode: diversity 4:2 / non-diversity 8:1 or 8:4 (SW configurable)

Wide bandwidth: from 150 up to 1160 MHz

Remote management and monitor of alarms thru Ethernet 10/100 base TX

Antenna booster supply toggled on each input independently

Voltage and current monitoring on each booster supply with alarm

Programmable attenuators on each inputs

Remote boost control (for gain/bandwidth) with a bidirectional data link thru coax(input BNCs)

light window where the user can enter their own text to identify the 8 areas

3. 규격 및 사양

Power supply	: AC connector 90÷264Vac / T2A, 47÷63Hz

Working frequency	: 150 ÷ 840MHz (MAT244),	150 ÷ 960MHz (MAT244X),	150 ÷ 1160MHz (MAT244X1)

Amplifier linearity	: ± 1 dB (typical)

“A” / “B” antenna input	: 8 BNC type connector

antenna output	: 4 BNC type connector

Impedance	: 50 Ω

Input/output Gain	: 7 dB (Combiner 8:1), OIP3=30dBm typ.

: 0 dB (Combiner 8:4), OIP3=24dBm typ.

: 7 dB (2 Combiners 4:2), OIP3=30dBm typ

Noise Figure	: 5.5dB (each channel)

Antenna booster powering	:+12Vcc /800mA MAX for ports 1A,1B[2x4:2	conf] or for port 1,5 [other configuration]

: +12Vcc / 230mA MAX (other ports)

Configuration/monitor interfaces	: 10/100 Base TX Ethernet port

Display	: 64 x 256 OLED (yellow)

Dimension	: Standard rack (aluminum) 19” / 1U.

Weight	: 3.7 Kg

* MAT244 동급이상품