*) 12-CHANNEL MIXING CONSOLE WITH MULTI-FX & RECORDING

1. 개요

본 기기는 아날로그 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Sturdy Metal Chassis

PRO DSP FX onboard with 16 presets

Stereo Recording and Playback via USB port

Balanced main output audio path from input to output

4 single control compressors

Mono channels provided with 3-band EQ. 2-band EQ on stereo channels.

Robust, compact and attractive design.

Designed and Engineered in Italy

Internal Universal Power Supply

3. 규격 및 사양

Electronic specifications

Frequency Response	: 20 Hz ~ 20 kHz

THD+N, 20dB gain, 0dBu out	: <0,02% A-Weighted

Processing

Dynamic Range	: > 85dB

Inputs

Channels	: 12

Mic	: 6

Gain Range	: 0 dB ~ -50 dB

Input Noise Level	: -124 dBu A-Weighted

Mic Inputs Impedance	: 14 kohm

Low Cut	: 80 Hz

Phantom Power +48V	: Yes

Mono Line	: 4

Gain Selection	: 20 dB ~ -30 dB

Line Input Impedance	: 21 kohm

HI-Z Line Inputs	: 1

HI-Z Line Inputs Impedance (Mohm): 1 Mohm

Stereo Line	: 4

Gain Selection	: 20 dB ~ -30 dB

Stereo Line Input Impedance (kOhm): 15 kohm

Input Connectors	: XLR, Jack, RCA

Outputs

Main MIX	: 1

Control Room	: Yes

FX Send	: 1

AUX Send	: 1

AUX Output	: 2

Group Out	: 1

Phones	: 1

Output Connectors	: XLR, Jack

Outputs specifications

Main Out Level	: 28 dBu

Aux Out Level	: 28 dBu

Group Out Level	: 28 dBu

Phones Out impedance (ohm)	: 150 ohm

Compressors

RCF Compressors	: n°4 Single Control Compressors on	Channels 1 to 4

EQ

Input Channels EQ	: 2 Shelving / 1 Generic

Description	: High: +/-15 dB @ 10 kHz Shelving	Mid: +/-15 dB @ 1,250 kHz Bell	Low: +/-15 dB @ 100 Hz Shelving

Auxiliary sends

AUX	: 1 PRE/POST

FX POST	: 1

Internal Effects

Send Effects	: 1

USB audio

USB Audio Interface	: Yes

Type	: B

Play trk	: 2

Rec trk	: 2

Supported Sample Rate	: 44.1, 48.0 kHz

Other features

Footswitch	: Yes

Electrical specifications

Power supply	: Internal

Voltage requirements	: 100 V - 240 V

Power consumption (MAX)	: 24 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Color	: Black

Size

Height	: 97 mm / 3.82 inches

Width	: 373 mm / 14.69 inches

Depth	: 355 mm / 13.98 inches

Weight	: 4.5 kg / 9.92 lbs

* F 12XR 동급이상품